The table 9-82 in VVC D6vE

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| ... | | | | | | |
| merge\_idx[ ][ ] | 0 | bypass | bypass | bypass | bypass | na |
| merge\_triangle\_split\_dir[ ][ ] | bypass | na | na | na | na | na |
| merge\_triangle\_idx0[ ][ ] | 0 | bypass | bypass | bypass | bypass | na |
| merge\_triangle\_idx1[ ][ ] | 0 | bypass | bypass | bypass | na | na |
| … | | | | | | |

Should be modified as:

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| ... | | | | | | |
| merge\_idx[ ][ ] | 0 | bypass | bypass | bypass | bypass | na |
| merge\_triangle\_idx0[ ][ ] | bypass | bypass | bypass | bypass | na |
| merge\_triangle\_idx1[ ][ ] | bypass | bypass | bypass | na | na |
| merge\_triangle\_split\_dir[ ][ ] | bypass | na | na | na | na | na |
| … | | | | | | |